RE: 19208 Parkside Street

Installation specifics as listed in contract

* Install IA (Imperial Armor) over Front Bay and flat of Hip Roof in back
* Install Oxford style shingle over Barrell roof in front of house and roof over side door going back to back yard.
* We are not doing any work with the roof deck on back 2nd story.
* Repair 1 foot of fascia on attic fan with hole in it
* Repair and Install fascia on Barrell roof as needed.
* Install Rustic Shingle over Back Bay.
* Install Rustic Shingle on the outside of attic fan where existing asphalt is.
* Remove 2 layers of asphalt, 1 layer of wood.